**ASSESSING THE SPATIAL VARIABILITY OF GROUND MOTION FOR MICROZONATION PURPOSES: THE CASE STUDY OF CAVEZZO MUNICIPALITY (ITALY)**

Lai1,2 C.G., Poggi3 V.\*, Famà1,2 A., Zuccolo1,2 E., Bozzoni2 F.\*, Meisina4 C., Boni4 R., Martelli5 L., Massa6 M., Mascandola6 C., Petronio3 L., Affatato3 A., Baradello3 L., Castaldini7 D., Cosentini8 R.M.

1Department of Civil and Architectural Engineering, University of Pavia, Italy

2European Centre for Training and Research in Earthquake Engineering, EUCENTRE, Pavia, Italy

3National Institute of Oceanography and Applied Geophysics, OGS, Trieste, Italy

4Department of Earth and Environmental Sciences, University of Pavia, Italy

5Servizio Geologico Sismico e dei Suoli, Regione Emilia-Romagna, Bologna, Italy

6National Institute of Geophysics and Volcanology, INGV, Milano, Italy

7 Department of Chemical and Geological Sciences, University of Modena and Reggio Emilia, Italy

8Department of Structural, Building and Geotechnical Engineering, Politecnico di Torino, Italy

\*Corresponding authors:

- Valerio Poggi, Researcher, Italian Institute of Experimental Oceanography and Geophysics, OGS, Trieste, Italy, [vpoggi@inogs.it](mailto:vpoggi@inogs.it)

- Francesca Bozzoni, Researcher, European Centre for Training & Research in Earthquake Engineering, Via Ferrata, 27100 - Pavia, Italy, [francesca.bozzoni@eucentre.it](mailto:francesca.bozzoni@eucentre.it)

**ABSTRACT**

~~In July 2017, an inter-institutional agreement was signed among the University of Pavia, EUCENTRE, the administration of Emilia-Romagna Region, the Province of Modena and the Municipality of Cavezzo to perform a microzonation study at the town of Cavezzo (Modena, Northern Italy). This research study was led as part of the European H2020 project LIQUEFACT, initiated in May 2016 with the main goal of establishing guidelines for the assessment and mitigation of damages to structures and infrastructures caused by earthquake-induced soil liquefaction. Within this framework, the municipality of Cavezzo was selected, among four European testbed territories, as case-study for mapping the liquefaction hazard at urban scale with the ultimate goal of drawing up a microzonation chart.~~

As part of the European H2020 project LIQUEFACT, an extensive level III microzonation study was performed at the town of Cavezzo (Modena, Italy), selected as test case representative of a typical territory susceptible to liquefaction hazard at urban scale. In this paper, we discuss the work carried out ~~in Cavezzo~~ to characterize the spatial variability of ground motion amplification due to local soil conditions in the municipality area.

A multi-disciplinary approach is presented, involving geotechnical engineers, geophysicists, geologists and seismologists from different institutions, with the goal of thoroughly characterizing the territory using complementary techniques ~~at different scales and~~ with different level of resolution and confidence. A considerable amount of geomorphological, geological, hydrogeological, seismological, geotechnical and geophysical investigations was collected and processed for the purpose. A GIS-based (Geographic Information System) platform was initially setup to manage the gathered data, which now includes the outcomes of about 1,000 geotechnical and geophysical tests. Such extended dataset was then used as primary constraint for the creation of a comprehensive pseudo-3d geotechnical and a seismo-stratigraphic model of the territory, consisting of a dense grid of one-dimensional vertical profiles to depict the variability of the soil properties over the area. The model was finally used as the input for linear-equivalent ground response analyses. For the calculation of the amplification factors, special emphasis was given to the treatment and propagation of the uncertainties of the model parameters, whose different realizations have been accounted though a logic tree approach.

1. **INTRODUCTION**

The seismic microzonation of a territory is the process that aims at identifying and mapping the subsoil seismic response and earthquake-induced phenomena of that territory. Typically, the spatial scale at which the zonation is performed is that of a municipality (urban scale) and it involves both the phenomenon of ground shaking amplification and ground instabilities. In Italy, the national reference document for seismic microzonation is the “Guidelines for Seismic Microzonation” (SM Working Group, 2015). It establishes criteria and operational instructions for the identification of areas subjected to ground amplification and ground instabilities (i.e. slope instability, soil liquefaction and ground failures) to guide the urban planning of local administrators. Similarly to the guidelines of seismic microzonation issued by the TC4-ISSMGE (1999), three levels of microzonation studies are identified: *level 1* is the *basic level* and it relies on gathering existing geologic, geomorphologic and hydrogeological data which are processed to roughly subdivide the investigated territory into a certain number of homogeneous zones where the expected seismic hazard intensity or risk of ground failure is uniform. ~~The resolution scale in grade 1 microzonation is low.~~ *Level 2* ~~on the other hand~~, is based on using existing geologic data and abaca containing coefficients for ground amplification. Non-invasive geophysical surveys are encouraged. *Level 3* is the most detailed level of microzonation. As such, it requires purposely-planned geotechnical and geophysical investigations as well as numerical ground response analyses, for a quantitative definition of seismic hazard and geological-geotechnical risks. Whereas level 1 and 2 microzonation are commonly performed in Italy, a level 3 study is restricted to few municipalities of special interest, given the considerable time and financial investment required.

One of the main goals of the H2020 European project LIQUEFACT 2016-2019 (<http://www.liquefact.eu/>) is the definition of objective criteria to assess liquefaction hazard at different geographic scales. ~~The project, initiated in May 2016 and ending in October 2019, also aims at addressing other risk-related aspects of liquefaction potential, including the impact to structures and infrastructures of earthquake-induced soil liquefaction as well as mitigation of liquefaction risk through ground improvement techniques.~~ LIQUEFACT Work Package 2, led by University of Pavia and EUCENTRE, deals with zonation of a territory both at continental (macro-zonation) and sub-municipal scale (micro-zonation). In this framework, four European testbed territories were selected as case-studies where to perform seismic microzonation for earthquake-induced liquefaction hazard. ~~The four target areas have been selected in Emilia-Romagna region (Northern Italy), Lisbon metropolitan area (Portugal), Ljubljana area (Slovenia) and in Marmara region (Turkey).~~ The territory of the Municipality of Cavezzo have been chosen as Italian case-study, since it experienced the 2012 seismic sequence occurred in Emilia-Romagna Region (e.g. Tertulliani et al. 2012, Locati et al. 2016, Rovati et al. 2016, etc.), where widespread liquefaction manifestations occurred (e.g. Martelli and Romani 2013, Fioravante et al. 2013, Lai et al. 2015, etc.). In this framework, an inter-institutional agreement was signed in July 2017 involving the University of Pavia, EUCENTRE, the administration of Emilia-Romagna region, the administration of the Province of Modena and the municipality of Cavezzo to perform a grade 3 microzonation study of the territory of Cavezzo, according with the Italian guidelines to support territorial and urban planning, named “Guidelines for Seismic Microzonation” (SM Working Group, 2015). Although the study was focused on the assessment of liquefaction hazard at urban scale, this paper presents a summary of the research activities carried out in performing the seismic microzonation of Cavezzo with special reference to ground shaking. In particular, the creation of a detailed seismo-stratigraphic model from the analysis of existing and newly acquired geotechnical and geophysical data will be illustrated. Special attention is given to the treatment and propagation of the uncertainties due to both the overall variability of the input data and that associated with data processing and modeling assumptions. The interdisciplinary nature of the conducted work is highlighted, discussing the adopted methodological approaches, the diversity of data calibration and the way these challenges have been collectively handled to create a unified yet comprehensive ground motion amplification model.

1. **GEOLOGICAL AND SEISMOTECTONIC SETTING**

Cavezzo municipality is located within the northern sector of the Modena province (Italy), on the right side of the Secchia River (**Figure 1**a). The study area sits within the western margin of the Po plain, a large foreland sedimentary basin originated by the progressive convergence of the Africa/Adria and Eurasia plates initiated during the late Cretaceous and still ongoing. Such compressional regime led to the development of large thrust and folds structures with roughly WNW-ESE trending, but of opposing vergence to the North and to the South of the longitudinal valley axis. Some of the southern buried structures have demonstrated to be still under active shortening, causing non-negligible historical seismicity, whose noticeable expression was the recent 2012 Emilia sequence.

The sedimentary infill of the Po plain consists of a thick sequence of sediments of Tertiary-Quatertiary age, from fine Pliocene muds to more course silt, sand and gravel alternations due to transition to continental deposition from the Pleistocene. Depositional sequence is heavily perturbed by the ongoing deformation process and the alternation of episodes of erosion and glaciation, which have generated several noticeable angular unconformities and gaps (Mascandola et al. 2019).

At local scale, Cavezzo is on the southern limb of the buried Mirandola antiform (Boccaletti et al., 2004; Martelli et al., 2017, **Figure 1**b). The lithostratigrafic succession of the area is composed by alluvial deposits ranging in thickness from around 130 m in the northern area to 280 m in the southern one (RER-ENI, 1998). The bedrock is constituted by interbedded marlstones and sands of the Pliocene and Lower Pleistocene “Argille Azzurre” Formation and Middle Pleistocene “Imola Sands” Formation (RER-ENI, 1998). The alluvial deposits in the Cavezzo area are characterized by interbedded fine silty-clayey soils with layers rich of peat and interbedded sands and silty sands. These surficial sediments were deposited by the Secchia River, whereas the deeper sand layers were deposited by the Po River (Castaldini, 1989).

From the morphological point of view, the study area is located in the alluvial plain of the Secchia River, ranging in elevation from 34 m a.s.l. in the southern and western sector to around 20 m a.s.l. in the northern part. It is worth noting that the highest topographic level is reached in correspondence of the modern artificial levees of the Secchia River, which raise about 7-8 m above the surrounding area (**Figure 2**). The study area includes different geomorphological features interpreted as floodplain, fluvial ridges and crevasse splays. The subsoil of Cavezzo is mainly characterized by silty-clayey sequences including channel-filling and crevasse splay sand layers (Pellegrini and Zavatti, 1980).

1. **METHODOLOGY**

A seismic response of the study area has been performed following four major steps, which are here summarized.

1. First, all existing geotechnical and geophysical measurements already available for the territory have been collected and organized in a comprehensive GIS database. The database has been subsequently extended with a number of new ad-hoc geophysical investigations on selected strategic locations.
2. A 3d geological/lithological model for the uppermost 30m was then constructed integrating boreholes and CPT data. The resulting model, extending over an area of approximately 27 km2, has been used for the identification of major surface lithological units (LU) and for the assessment of the liquefaction potential.
3. Next, a large-scale seismo-stratigraphic model was developed based on a combination of active and passive seismic data, including single measurement and 2d arrays ambient vibration analyses and high-resolution P and S reflection prospecting. The model consists of a grid of 2,984 nodes with 0.001 degrees spatial resolution (about 100 meters). For each grid node, a set of 11 complementary 1D vertical seismo-stratigraphic S-wave velocity profiles was identified to account for the uncertainties associated to the investigations. The resulting pseudo-3d model extends down to about 200m depth.
4. The previous geological/lithological and seismo-stratigraphic models were finally combined for the calculation of the seismic amplification factors through numerical ground response analyses using a stochastic approach. Seven spectrum-compatible accelerograms defined for 475, 975, and 2,475 years return periods were selected as input motion (referred to outcropping rock conditions). The 1d soil amplification function was then computed for each grid node and each velocity profile using a linear-equivalent soil constitutive model, for a total of 229,768 analyses. The different amplification results were finally combined using the logic-tree approach to rationally account for the epistemic uncertainty associated to the velocity model and the reference input variability.

In the following sections, the different steps of the proposed methodology are discussed in details.

1. **GROUND CHARACTERIZATION DATASET**

To carry out ground response analyses, an accurate knowledge of the geotechnical characteristics of the shallow subsoil at the site is required. At this purpose, the territory of Cavezzo was thoroughly characterized from geomorphological, geological, hydrogeological, seismological, geotechnical and geophysical viewpoints.

As a start, existing data retrieved from trench pits, boreholes, piezometric, in situ and laboratory geotechnical and geophysical investigation campaigns were gathered. **Figure 3a** shows the existing data available for ground characterization of the territory of Cavezzo before the LIQUEFACT project started. Based on the quality and quantity of the retrieved existing data, then, complementary ground investigation campaigns were purposely devised (**Figure 3b**). **Table 2** includes the type and number of tests adopted for the ground characterization of the territory of the Cavezzo Municipality. In-situ geotechnical investigations included: cone penetration tests with acquisition of the excess pore water pressure (CPTu) and the shear wave velocity Vs (SCPTu), standard penetration tests (SPT) and drilling of boreholes. Laboratory tests were also performed on undisturbed soil samples retrieved with the standard Osterberg sampler and the innovative gel-push technique for coarse-grained materials (Cubrinovski et al., 2016).

A number of non-invasive geophysical tests were also performed. These included 3D electric tomography, active and passive seismic surveys. In this regard, ~~fundamental was the contribution of~~ the National Institute of Geophysics and Volcanology (INGV Milano) and the National Institute of Oceanography and Applied Geophysics (OGS, Trieste)~~, who~~ respectively led a large-scale ambient vibration survey (including single-station H/V spectral ratio and 2D array measurements) and a high-resolution P/S reflection seismic survey. Such combined geophysical prospecting allowed illuminating large volumes of soils and at great depths (> 200 m from the ground surface) to identify the location of the seismic bedrock, while providing a mean to correlate the results obtained at different locations from the conventional geotechnical tests.

All data gathered on the subsoil of Cavezzo were organized into a purposely-developed GIS database, which now includes the data of more than 1,000 geotechnical and geophysical tests, as shown in  **Figure 3b**. Data of both 1m and 5m resolution DEM were also included.

1. **MODELING OF THE SUBSOIL**
   1. *Geotechnical/lithological model*

Based on a joint analysis of stratigraphic, lithological and geomorphological data, the territory of Cavezzo was tentatively subdivided into a number of geologically homogenous zones (MOPS), identified using an approach described in detail in a previous work by Meisina et al. (2019), which includes also the typical stratigraphic logs derived for each zone. Specifically, 9 main geological domains have been identified based on joint stratigraphic analysis of boreholes and water wells and from the interpretation of CPTu/CPT tests. These domains were used to separate zones of supposedly homogeneous lithological and genetic depositional characteristics (**Figure 4**). For the stratigraphic interpretation of CPTu/CPT data, it was used a correction of Soil Behaviour Index (Ic, Robertson 2009) calibrated using the available CPTu tests and boreholes data (Meisina et al. 2019) in order to identify the mixture layers falling within the transition zone of the reference chart (Robertson, 2009).

* 1. *Seismo-stratigraphic model*

The previously described lithological model was preliminary to the definition of the seismo-stratigraphic idealization of the subsoil, which was obtained by integrating the existing geophysical data (mostly from shallow MASW investigations) with purposely-planned active and passive seismic acquisitions. In the following, the different steps for the creation of the seismo-stratigraphic model are described.

* + 1. *Calibration of the reference velocity model*

As a first step, assuming a smooth lateral variability of the geophysical parameters over the investigated area, a set of reference one-dimensional seismic velocity profiles were established at selected representative locations. The different profiles were derived from two independent although complementary geophysical approaches, based respectively on the array analysis of ambient vibrations (hereinafter called the INGV model) and from the processing of high-resolution reflection of P/S seismic data (hereinafter called the OGS model).

Concerning the analysis of ambient vibration data, the velocity profiles were obtained from combined inversion of multi-component surface wave information (Poggi and Fäh. 2010). Love and Rayleigh velocity dispersion curves were first derived using the high-resolution frequency-wavenumber analysis on the three-component of motion (3CFK) as proposed by Poggi and Fäh (2010). This technique is beneficial in that it allows an efficient separation of the transversal (Love) and radial (Rayleigh) surface wave motion from the horizontal components, providing the dispersion information of both wave types and, at the same time, an unbiased estimate of the Rayleigh ellipticity (or polarization) function within the resolved frequency band. The one-dimensional seismic velocity profile is then obtained by combined inversion of Love and Rayleigh wave dispersion, including higher modes, the Rayleigh wave polarization function and fundamental frequency of resonance of the site (f0) from H/V analysis. The software Dinver (Wathelet et al., 2008) is used to perform inversion though an enhanced version of the neighborhood algorithm. The use of Love wave dispersion curves, which is generally uncommon, has the particular advantage to provide a unique constraint to the S-wave velocity of the medium. In combination with Rayleigh wave dispersion, then, it allows a more reliable estimation of the seismo-stratigraphic model. Complementary, the OGS velocity model has been derived from interval velocity analysis of P- and S-wave reflection seismic (see Petronio et al. 2018 for more details).

The two seismic techniques have shown to produce consistent results down to about 100 m depth from the ground surface, while some deviations were observed at larger depths (**Figure 6**). Such discrepancy is likely due to the intrinsic limitations of passive seismic analysis, whose resolution decreases progressively with increasing wavelength and investigated depth. On the contrary, seismic reflection methods generally provide a more accurate imaging of the profile, particularly on the layer interfaces, though at the expense of a higher implementational cost. In the present case, the two sets of velocity profiles have been considered both equally reliable and representative of the epistemic uncertainty of the reference seismo-stratigraphic models. Such variability is accounted for in the data processing by means of a logic-tree calculation approach.

* + 1. *Soil variability of the study area*

In a subsequent step, at each point of the pseudo-3D model the shear wave velocity profiles have been adjusted to match the observed variability of both the shallow subsoil and the deepest resonating layer interface (which was assumed to be the local seismic bedrock). To constraint the shallow portion of the velocity model, a map of the Vs30 variability was first obtained from existing MASW analyses from 83 previous surveys available for the study area. It should be noted that being the results from available MASW data heterogeneous (e.g. they were obtained from different contractor and using different processing schemes), it was decided to homogenously reassess the VS30 of each measurement by means of a simplified procedure as proposed by Brown et al. (2000) and further developed by Martin and Diehl (2004) and Albarello and Gargani (2010) (see also Comina et al. 2011 for clarifications). In short, the VS30 at each site was obtained empirically from the Rayleigh wave dispersion curve (**Figure 7**A) by extracting the phase velocity corresponding to a wavelength (λ) of 40 m, which provided estimates of VS30 (**Figure 7**B) comparable with those obtained from independent processing.

Spatial interpolation of the VS30 values was subsequently performed using widely used geostatistic algorithm, i.e. ordinary Kriging (Isaaks and Srivastava, 1989). This provided a mean shear wave velocity and the corresponding residual uncertainty at each point of the interpolated grid. Finally, at each location of the gridded model, the reference velocity profiles have been adjusted to match the interpolated VS30 value from MASW analysis. The adjustment was performed by applying a depth-dependent velocity correction factor, whose effects progressively decreases with the increase of depth, following a negative exponential function. This ensure that the observed shallow variability of VS does not sensibly impact the seismo-stratigraphic model at large depth.

* + 1. *Mapping the seismic bedrock*

The variability of the seismic bedrock was obtained using an adaptation of the procedure proposed by Poggi et al. (2012), based on Rayleigh wave ellipticity peak matching.

As starting point, a map of the fundamental frequency of the area was created by interpolation of 26 f0 values from single station ambient vibration measurements obtained using horizontal-to-vertical-ratio spectral analysis (e.g. Nogoshi & Igarashi 1971; Nakamura 1989; Haghshenas et al. 2008). Consistently with the procedure used to map shallow velocity variability, spatial interpolation of the sparse f0 values was performed using ordinary Kriging, accounting also for the associated uncertainty.

Subsequently, the one-dimensional velocity profiles at each grid point of the seismo-stratigraphic model have been adjusted to match the observed (thus interpolated) resonance frequencies. However, in contrast to what was previously done to account for Vs30 variability, in this case the adjustment was not performed directly on velocity, but by migrating the layer’s interface depth till a satisfactory match was found. We adopted a migration coefficient proportional to depth, with a large impact on the deep layer interfaces, while leaving substantially unmodified the uppermost portions of the velocity profile. This approach has the advantage to minimize the discrepancy of the adjusted velocity profiles to the original input constraints (e.g. surface wave dispersion, Vs30).

The resulting geophysical bedrock agrees with the expected geological features of the area, with a moderate North-South trend, related to the geometry of the nearby Mirandola anticline structure, although with a noticeable irregularity in a small region in the central part of the model.

* 1. *Final geotechnical-seismic model*

The final geotechnical-seismic model of the area of study was defined starting from the pseudo-3D seismo-stratigraphic model, consisting of 10 VS INGV profiles each with an associated weight of 0.05 (overall weight equal to 0.5), and an OGS VS profile from seismic reflection survey to which a weight of 0.5 was associated. Each independent 3D model consisted of 2,984 1D VS-profiles at each node of a reference grid that covers the territory of Cavezzo. Therefore, a total of 32,824 VS profiles (2,984x11) were defined and used for ground response analysis. Furthermore, for each profile a unique seismo-geotechnical model was created by merging the soil properties of the geological/lithological and geophysical models. At this purpose the 9 geologically homogeneous zones discussed in § 3.2 were used jointly with their associated uncertainties. In each homogeneous zone, the nodes of the reference grid falling within its boundaries have been identified for each layer of 11 seismo-stratigraphic models and a statistical analysis of the corresponding thicknesses was performed. Since the assessment of ground amplification was performed using 1D linear-equivalent analysis, a purposely-devised calibration of the shear modulus and damping ratio decaying curves was accomplished following the methodology proposed by Darendeli (2001) coupled with the experimental data from laboratory tests performed in the area of study in December 2017 (**Figure 8**).

1. **SEISMIC RESPONSE FOR MICROZONATION**
   1. *Definition of the reference seismic input and its variability*

Emilia-Romagna region issued in 2015 (DGR n.2193) regional guidelines to support territorial and urban planning, which are consistent with the national “Guidelines for Seismic Microzonation” (SM Working Group, 2015). These regional guidelines provides 3 real accelerograms recorded on outcropping bedrock to be used as input motion for ground response analyses. It must be noted, however, these signals are not independent from each other; in addition, they are referred only to the 475 years return period. Thus, they are unsuitable to the scope of the study. Consequently, the seismic hazard at the site was defined in terms of seismo- and spectrum- compatible natural accelerograms for three return periods (475, 975 and 2475 years). Spectrum-compatibility was enforced with reference to 5% damped, elastic acceleration response spectra (horizontal component of motion) referred to stiff ground conditions specified by the current Italian building code (NTC, 2018).

Table 1 summarizes, for each considered return period, the parameters required to define the elastic response spectra for soil class A with reference to Cavezzo: ag is the horizontal peak ground acceleration on a rigid reference site, F0 is the amplification factor of the horizontal acceleration spectrum and TC\* is the upper limit of the oscillator period of the constant spectral acceleration branch.

For each return period, a suite of 7 independent natural accelerograms recorded on free-field rock ground conditions, spectrum-compatible with the elastic response spectrum defined by the NTC (2018) for the territory of Cavezzo was selected. The selection was made using an updated version of ASCONA computer program (Corigliano et al., 2012), which provides a set of strong motion recordings satisfying specific seismological criteria (e.g., magnitude and distance ranges, spectral shape), with the additional requirement of being compatible with a target spectrum (in this case, the elastic acceleration response spectrum prescribed by the current Italian building code), in a specified oscillator period range (in this case, from 0.15 s to 2 s). Regarding record scaling, the PEER (2010a, 2010b) approach was adopted. Among different accelerogram sets that satisfy the requirements, the set returned by ASCONA is the one characterized by the minimum average deviation of the average response spectrum (of the 7 accelerograms) with respect to the target spectrum.

* 1. *Ground response analyses*

One-dimensional ground response analyses were carried out in Cavezzo territory using SHAKE91 (Schnabel et al., 1972; Idriss and Sun, 1992) coupled with the linear-equivalent soil constitutive model. The analyses were conducted for 3 return periods, 7 accelerograms, 2,984 nodes of the reference grid for which the geotechnical-seismic pseudo 3D (P3D) model was defined and 11 VS profiles, for a total of 229,768 analyses. For each analysis, amplification factors (Fi) in terms of peak ground acceleration, Housner intensity ratio (computed considering 4 different oscillator period ranges) and acceleration response spectrum integral ratio in the spectral interval between 0.1s and 0.5s were computed. At each node of the grid and for each return period, the Fi values computed from the 7 accelerograms and 11 VS profiles were averaged as follows:

|  |  |
| --- | --- |
|  | (1) |

where w\_accj is the weight of the accelerogram, assumed to be the same for all accelerograms (w\_accj=1/7), w\_modk is the weight of the P3D model (w\_modk=0.05 for each of the 10 models based on INGV data and w\_modk=0.5 for the OGS model), while Fijk is the amplification factor Fi associated with the j-th accelerogram and the k-th P3D model.

It should be remarked that the suitability of 1D modelling in Cavezzo, mostly characterized by a stack of homogeneous flat and parallel layers with a negligible slope of the bedrock roof (around 5% in its steepest part), was confirmed by a 2D ground response analysis performed with QUAD4M (Hudson et al., 1994). In fact, the 2D analyses, which were performed with reference to a 110 m – long section crossing Cavezzo along the NS direction (i.e. the one with the largest variability in the sloping of the bedrock roof), allowed to obtain amplification factors similar to those obtained by 1D analyses. From the comparison of the results from 1D and 2D ground response analyses it was inferred that for the frequencies of interest in the microzonation study, 2D effects are negligible.

1. **SEISMIC RESPONSE RESULTS**

**Figure 9** shows ~~the map of~~ the ground motion amplification factors computed for the municipality of Cavezzo for the 475 years-return period. In agreement to the 2015 (DGR n.2193) Emilia Romagna guidelines, the amplification factors (Fi) have been computed in terms of both peak ground acceleration (FPGA, expressed as PGA/PGA0 ratio) and Housner intensity ratio (expressed as SI/SI0), computed for 3 different oscillator period ranges: FH0.1-0.5s, FH0.5s-1.0s, FH0.5-1.5. The terms PGA0 and SI0 are respectively the peak ground acceleration and Housner intensity related to the reference input motion. According to expectation, the largest amplification factors are experienced in the northern part of the municipality, in the proximity of the culmination of the Mirandola anticline~~, which is clearly visible in the four maps~~. Moreover, it is interesting to note that these maps clearly reflect even the homogeneous zones defined based on lithological and genetic depositional environment. The boundaries of these areas can be seen in trend with the values of the amplification factors. For instance, this fact is clearly visible in the high period range, namely FH0.5s-1.0s (bottom left) and FH0.5-1.5 (bottom right); lower values were obtained in homogeneous zones named 3 and 4 showed in **Figure 4**.[EXTEND THIS AS FOR POINT 9 OF 2ND REVIEWER]

1. **DISCUSSION AND CONCLUSIONS**

From the results of ground amplification analyses it is readily apparent the correlation between the spatial variability of surface ground motion within Cavezzo territory and the characteristics of the adopted seismic-geotechnical and seismo-stratigraphic models. This clearly highlights the importance of the interplay and complementarity among different methodological approaches and spatial resolution scales characterizing a seismic microzonation study when tackled from a geological, geophysical, seismological and geotechnical prospective. The challenge to succeed in such a study consists in explicitly recognizing its intrinsic multi-disciplinary nature in pursuing the goal of defining a unified subsoil model that harmonizes coherently the different scales at which it can be visualized.

It must be remarked however that the procedure illustrated in this article, strictly applies to situations where the geological setting is such that a smooth spatial variation of the subsoil properties over the territory, is an acceptable approximation, at the points of the calculation grid. In case of evident 2D/3D response, the use of more advanced numerical models will be unavoidable. Nonetheless, such condition must be evaluated carefully on a case by case scenario, e.g. by a preliminary inspection of the H/V spectral ratio variability across the area, in order to justify the increased investment required for such advanced and computationally very expensive analysis. So far, very few attempts are available in the literature to objectively quantify the possibility of 2D/3D morphological effects, which makes this subject an open field of research.

It is also important to underline that ground response analyses were conducted using a linear equivalent soil constitutive model. This approach of adopting one-constituent, equivalent-linear viscoelastic rheology for the soil is inadequate to correctly reproducing the seismic response of geomaterials exhibiting strong nonlinearities in the hydro-mechanical behaviour. An example is constituted by liquefiable soils, which require ground response analyses to be more correctly conducted using effective stress-based soil constitutive models.

Finally, an advancement of the current achievements in the seismic microzonation of Cavezzo territory could be represented by a complete randomization of all soil parameters and other input data for ground response analyses so to produce a fully stochastic set of amplification factors.

**ACKNOWLEDGMENTS**

This research has been carried out within the framework of the European LIQUEFACT project. The LIQUEFACT project has received funding from the European Union’s Horizon 2020 Research and Innovation Programme under Grant Agreement No. 700748. This support is gratefully acknowledged by the authors. The study herein presented has been carried out by a multi-disciplinary working group. In this framework, the authors would like to acknowledge:

* Sonia Lorini, Daniele Conca, Roberta Bonì, Alì G. Ozcebe, Massimiliano Bordoni, Pina Persichillo, Juan C. Gòmez Zapata, Giuseppe Cerra, Giacomo Perotti and Simone Ciaffaroni from University of Pavia;
* Daniela Fontana, Stefano Lugli and Alessandro Ghinoi from University of Modena and Reggio Emilia;
* Sara Lovati, Simona Carannante, Paola Morasca, Ezio D’Alema, Gianlorenzo Franceschina and Antonio Gomez from INGV (Milan Section);
* Alfio Barbagallo, Gino Cristofano and Daniele Sorgofrom OGS;
* Giulio Ercolessi from Emilia-Romagna Region;
* the Major of the Cavezzo Municipality and the technical staff in particular Agnese Malagoli.

**REFERENCES**

Boccaletti, M., Bonini, M., Corti, G., Gasperini, P., Martelli, L., Piccardi, L., Severi, P. & Vannucci, G. 2004: Carta sismotettonica della Regione Emilia-Romagna, scala 1:250.000. Note illustrative. Regione Emilia-Romagna–SGSS, CNR-IGG. SELCA, Firenze.

Castaldini, D. 1989. Evoluzione della rete idrografica centropadana in epoca protostorica e storica. Atti Conv. Naz. Studi "Insediamenti e viabilità nell'alto ferrarese dall'Età Romana al Medioevo". Cento 8-9 May 1987 Acc. delle Sc. di Ferrara, 115-134, Ferrara.

Corigliano, M., Lai, C.G., Rota, M., Strobbia, C.L. (2012). “ASCONA: automated selection of compatible natural accelerograms”. Earthquake Spectra, 28(3): 965-987.

Cubrinovski, M., Stringer, M., Haycock, I. (2016). Experience with gel‐push sampling in New Zealand. <http://www.nzgs.org>.

Fioravante V, Giretti D, Abate G, Aversa S, Boldini D, Capilleri PP et al. (2013). Earthquake geotechnical engineering aspects of the 2012 Emilia-Romagna earthquake (Italy). Proceedings of the 7th international conference on case histories in geotechnical engineering, Chicago, Illinois, USA.

Haghshenas, E., Bard, P.-Y., Theodulidis, N. & SESAME WP04 Team, 2008. Empirical evaluation of microtremor H/V spectral ratio, Bull. Earthq. Eng., 6(1), 75–108.

Hudson, M.B., Beikae, M., Idriss, I.M. (1994). “QUAD4M, a Computer Program to Evaluate the Seismic Response of Soil Structures Using Finite Element Procedures and Incorporating a Compliant Base Center for Geotechnical Modeling”, Department of Civil and Environmental Engineering, University of California, Davis.

Idriss, J., Sun, J.I. (1992). SHAKE91 - a computer program for conducting equivalent linear seismic response analyses of horizontally layered soil deposits. University of California, Davis, USA.

Isaaks EH, Srivastava RM (1989). An Introduction to Applied Geostatistics. Oxford University Press, New-York.).

Lai CG, Bozzoni F, Mangriotis MD, Martinelli M (2015). Soil liquefaction during the May 20, 2012 M5.9 Emilia earthquake, Northern Italy: field reconnaissance and post-event assessment. Earthquake Spectra, 31(4), 2351-2373.

Lai, C.G., Meisina, C., Bozzoni, F., Conca, D., Famà, Özcebe, A.G., Zuccolo, E., Bonì, R., Poggi, V., Cosentini, R.M. (2019). Mapping the liquefaction hazard at different geographical scales. Proceedings 7th International Conference on Earthquake Geotechnical Engineering, 7ICEGE, Rome, Italy, 17-20 June, 2019.

Lo Presti, D., Sassu, M., Luzi, L., Pacor, F., Castaldini, D., Tosatti, G., Meisina, C., Zizioli, D., Zucca, F., Rossi, G., Saccorotti, G., & Piccinini, D. 2013. A Report on the 2012 Seismic Sequence in Emilia (Northern Italy). International Conference on Case Histories in Geotechnical Engineering. 3.

Locati M., Camassi R., Rovida A., Ercolani E., Bernardini F., Castelli V., Caracciolo C.H., Tertulliani A., Rossi A., Azzaro R., D’Amico S., Conte S., Rocchetti E. (2016): DBMI15, the 2015 version of the Italian Macroseismic Database. Istituto Nazionale di Geofisica e Vulcanologia. doi:http://doi.org/10.6092/INGV.IT-DBMI15

Lugli S., Marchetti Dori S., Fontana D. 2007. Alluvial sand composition as a tool to unravel the Late Quaternary sedimentation of the Modena Plain, northern Italy. In: Arribas, J., Critelli, S., Johnsson, M.J. (Eds.), Sedimentary Provenance and Petrogenesis: Perspectives from Petrography and Geochemistry. Geological Society of America Special Paper, 420, 57-72.

Martelli L, Romani M (2013). Microzonazione sismica e analisi della condizione limite per l’emergenza delle aree epicentrali dei terremoti della pianura emiliana di maggio-giugno 2012 (Ordinanza del commissario delegato n. 70/2012), Relazione Illustrativa (in Italian); <http://ambiente.regione.emilia-romagna.it>

Martelli, L., Bonini, M., Calabrese, L., Corti, G., Ercolessi, G., Molinari, F. C., Piccardi, L., Pondrelli, S., Sani, F. & Severi, P. 2017. Carta sismotettonica della Regione Emilia-Romagna e aree limitrofe. Note illustrative. Regione Emilia-Romagna, Servizio geologico, sismico e dei suoli. D.R.E.AM. Italia.

Meisina, C., Bonì, R., Bordoni, M., Lai, C.G., Bozzoni, F. et al. 2019. 3D Geological model reconstruction for liquefaction hazard assessment in the Po Plain. Proceedings 7th International Conference on Earthquake Geotechnical Engineering, 7ICEGE, Rome, Italy, 17-20 June, 2019

Nakamura, Y., 1989. A method for dynamic characteristics estimation of subsurface using microtremor on the ground surface, Quart. Records Railway Tech. Res. Inst., 30, 25–33.

Nogoshi, M. & Igarashi, T., 1971. On the amplitude characteristics of microtremor, Part II, J. seism. Soc. Japan, 24, 26–40.

NTC (2008). Norme Tecniche per le Costruzioni. Decreto del Ministero delle Infrastrutture del 14 gennaio 2008. Gazzetta Ufficiale, n. 29 del 4 febbraio 2008, Supplemento Ordinario n. 30, www.cslp.it, Istituto Poligrafico e Zecca dello Stato, Roma (in Italian).

NTC (2018). Norme tecniche per le costruzioni. Ministero delle Infrastrutture e dei Trasporti, Decreto Ministeriale del 17 gennaio 2018, Supplemento ordinario alla G.U. n. 8 del 20 febbraio 2018 (in Italian).

Paolucci E, Albarello D, D’Amico S, Lunedei E, Martelli L, Mucciarelli M and Pileggi D (2015) A large scale ambient vibration survey in the area damaged by May–June 2012 seismic sequence in Emilia Romagna, Italy. Bull Earthquake Eng 13:3187–3206. DOI 10.1007/s10518-015-9767-5.

PEER (2010a). Technical report for the PEER ground motion database web application-Beta Version-October 1, 2010. Pacific Earthquake Engineering Research Center (PEER).

PEER (2010b). User’s Manual for the PEER ground motion database web application-Beta Version-October 1, 2010. Pacific Earthquake Engineering Research Center (PEER).

Pellegrini, M. & Zavatti, A. 1980. Il sistema acquifero sotterraneo tra i fiumi Enza, Panaro e Po: alimentazione delle falde e scambi tra falde, correlazioni idrochimiche”. Quaderni IRSA, 51(1), Roma.

Petronio L., Affatato A., Baradello L., Barbagallo A., Cristofano G., Sorgo D., Lai C.G., Poggi V., 2018. Shear wave seismic reflection survey in the 2012 Emilia epicentral area. 38th GNGTS, Bologna, Italy.

Poggi, V. and Fäh, D., 2010. Estimating Rayleigh wave particle motion from three-component array analysis of ambient vibrations. Geophys. J. Int., Volume 180, Issue 1, 251-267.

Poggi, V., Fäh, D., Burjánek, J. and Giardini, D., 2012. The use of Rayleigh wave ellipticity for site-specific hazard assessment and microzonation. An application to the city of Luzern (Switzerland). Geophys. J. Int., Volume 188, Issue 3, 1154-1172.

RER–ENI. 1998. Riserve idriche sotterranee della Regione Emilia-Romagna. G. M. Di Dio. Regione Emilia- Romagna, ENI Agip Divisione Esplorazione e Produzione. S.EL.CA., Firenze, pp 120.

Rovida A., Locati M., Camassi R., Lolli B., Gasperini P. (eds) (2016) CPTI15, the 2015 version of the Parametric Catalogue of Italian Earthquakes. Istituto Nazionale di Geofisica e Vulcanologia. doi:http://doi.org/10.6092/INGV.IT-CPTI15

Schnabel, P.B., Lysmer, J., Seed, H.B. (1972). SHAKE: A computer program for earthquake response analysis of horizontally layered sites. Rep. No. EERC 72-12, EERI, Berkeley, Calif.

SM Working Group (2015). Guidelines for Seismic Microzonation”. Conference of Regions and Autonomous Provinces of Italy – Civil Protection Department, Rome, 2015.

TC4-ISSMGE [1999]. Manual for Zonation on Seismic Geotechnical Hazards (Revised Version). Technical Committee for Earthquake Geotechnical Engineering, TC4, ISSMGE. Published by The Japanese Geotechnical Society. ISBN 4-88644-809-7.

Tertulliani A., Arcoraci L., Berardi M., Bernardini F., Brizuela B., Castellano C., Del Mese S., Ercolani E., Graziani L., Maramai A., Rossi A., Sbarra M., Vecchi M. (2012): The Emilia 2012 sequence: a macroseismic survey. In “2012 EMILIA EARTHQUAKES”, Annals of Geophysics, 55, 4, 2012; doi: 10.4401/ag-6140.

Wathelet, M., Jongmans, D., Ohrnberger, M. et al. (2008). Array performances for ambient vibrations on a shallow structure and consequences over V s inversion. J Seismol 12, 1–19.

**TABLES**


**Table 1** Parameters adopted for the definition of the seismic hazard in Cavezzo, according with NTC (2018).

|  |  |  |  |
| --- | --- | --- | --- |
| **Return period (years)** | **ag (g)** | **F0 (-)** | **Tc\* (s)** |
| 475 | 0.151 | 2.588 | 0.270 |
| 975 | 0.202 | 2.535 | 0.276 |
| 2475 | 0.290 | 2.436 | 0.291 |


**Table 2** Type and number of tests adopted in this study for the ground characterization of the territory of the Municipality Cavezzo.

|  |  |
| --- | --- |
| **Testing types** | **Number** |
| Geotechnical in situ tests  *(boreholes; Cone Penetration Tests, CPT; Standard Penetration Tests, SPT; Flat Dilatometer Tests, DMT, etc.)* | 502 |
| Geophysical tests  *(seismic reflection, Multichannel Analysis of Surface Waves, MASW, H/V, Extended Spatial Autocorrelation, ESAC; Refraction Microtremor ReMi; Electrical resistivity tomography ERT, etc.)* | 409 |
| Geotechnical laboratoy tests  *(triaxial tests, resonant column tests, etc.)* | 73 |

**FIGURES**




**Figure 1.** a) Geographical location of the study area. b) Localization of the geological cross section. c) Geological section AA’ (modified from Paolucci et al 2015).



**Figure 2.** Main geological and geomorphological features of the area of Cavezzo (modified from Meisina et al., 2019).


|  |
| --- |
|  |
|  |
|  |

**Figure 3.**Location of the previously available (a) and newly acquired geophysical (b) and geotechnical (c) analyses performed on the study area. The manifestations of soil liquefaction occurred in 2012 sequence (black dots) and 1m resolution digital elevation model are superimposed. Modified from Lai et al. (2019).




**Figure 4.**Map of 9 homogenous geological zones (MOPS) defined for Cavezzo municipality. Modified from Meisina et al. (2019), which we refer for a detailed description of the zonation process.


|  |
| --- |
| A) |
| B) |
| C) |




**Figure 5.**Comparison between empirical and modelled Love and Rayleigh dispersion curves obtained respectively from three-component f-k analysis of ambient vibration array data and the best fitting inverted velocity models.





**Figure 6.** Comparison between two sample models from surface wave inversion of ambient vibration data (acquired by INGV) and from high-resolution P/S seismic reflection survey (OGS). The models show an overall good match down to a depth of about 140m, where an interface assumed to represent the seismic bedrock is located. Velocity is progressively mismatching the deeper layers.





**Figure 5:** Pseudo-3D model developed starting from seismic data acquired from old and new geophysical surveys using the combined inversion of multi-component surface wave datasets based on a joint interpretation of travel-times, dispersion and polarization data. The plot shows the geometry of the layer’s interfaces, sampled at each of the 2.984 nodes of the grid with a 0.001 degrees spatial resolution (about 100 meters).


A)

B) 

**Figure 7.** (A) Rayleigh wave dispersion curves form MASW analysis available for the territory (in black). Mean (red dots) and standard deviation (white dots) of the distribution is also presented to show the overall variability. (B) Distribution of the VS30 values obtained from the λ40m empirical approximation.



**Figure 8***.* Calibration of shear modulus and damping ratio decaying curves as proposed by Darendeli (2001) using data from laboratory tests performed in December 2017 in Southern area of Cavezzo municipality.



**Figure 9.** Map of amplification factors computed for Cavezzo considering the 475-years return period. Top left: PGA; Top right: Housner intensity ratio (0.1s≤T≤0.5s); Bottom left: Housner intensity ratio (0.5s≤T≤1.0s); Bottom right: Housner intensity ratio (0.5s≤T≤1.5s). The 9 homogenous geological zones (MOPS) shown in Figure 4 and defined for Cavezzo municipality are superimposed.

acc.pdf

spettro-comp.pdf